**FORM I**

**[See Rule 3(L)]**

**Form Of License For Manufacture Of, Commencement Of Carrying On Business As A Manufacture Of A Dangerous Machine.**

Licence No \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Whereas M/s \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ has/have

(give full address)

applied for a licence for commencement of/carrying onbusiness as a manufacturer of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(here specify which dangerous machine)

And whereas the Controller is satisfied that the condition specified in section 9(4)(a) or, as the case may, be, 9(4)(b) has been complied with.

Now, there fore in exercise of' the powers, conferred by section 9 of' the Act licence is granted/ renewed to M/s \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ for a period of five years to commence/carry on business as a manufacturer of' the :

1.

2.

3.

(Give name of machine and trade name with brief description and overall dimensions)

This licence is issued subject to the following conditions:-

(1) The manufacturer shell ensure that the machine and every part thereof complies with the standards specified by rule 4 of' the Dangerous Machines (Regulation) Rules.1984.

(2) Without prejudice to the generality of condition No.(1) above the Manufacture shall ensure that the following parts are secured by safeguard of substantial construction:--

(a) The prime-mover and every part thereof'.

(b) The transmission machinery and every part thereof.

(c) Every other dangerous part such as rollers, blowers, elevators andthe like.

(3) The manufacturer shall clearly and legibly provide the machine with danger signals indicating the point beyond which nolimb shall be inserted for thepurpose of feeding the machine or for any other purpose while the machine is in operation.

(4) The manufacturer shall ensure that the following particulars are legibly and conspicuously marked orinscribed onevery dangerous machine by Such method as would makeit indelible namely--

(a) The direction of the rotation and the number of rotations per minutes

(b) Its power requirements: and

(c) The nameand correct address of the manufacturer, the year of manufacture and the date, number and other particulars of the licence of the manufacturer.

(5) Every manufacturer shall supply along with eachdangerous machine a manualcontaining general instructions regarding the operation of such machine, and shall also include therein such cautions as may be prescribed.

(6) Before transferring the possession of the machine whether by sale, lease, hire or otherwise, the manufacturer shell deliver to the person acquiring the machine a declaration to the effect that the machine conforms to the standards laid down by or under this Act and also complies, in all respects with the provisions of the Act and the rules and orders made there under.

(7) Failure to comply with the conditions specified above or of any provision of the Act or rule or order made there under will make this licence liable to suspension/cancellation as provided in section 10.

[N.B All references to the Act or any section thereof are references to the Dangerous Machines (Regulation) Act- 1983 (35 of 1983), or the relevant section thereof]

Granted this \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 19 \_\_\_\_\_\_\_\_

Place:

Designation

Date:

(Seal)